25.02.2023

Card design B

Simple BS calculation:

BRC old :6103.515 hz t = 163.84 uSec

BRC new:3051 hz t = 327.76 uSec

327760nSec /20 = 16384 steps of 20nSec

¾ steps =(16384/4)x3 = 12288

DESIGN CARD B

Simple BS

BS filter

Data organizer

Rgb